{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["激光与通信类","电子类","Sheet3"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"激光与通信类","index":0,"n_rows":133,"n_cols":6,"rows_kept":133,"merged":[[0,0,1,5],[3,0,3,5],[4,0,4,5]],"flags":["formulas_cached_only"]}
["电子工程学院实训耗材采购清单、技术规格及要求"]
[]
[]
["投标文件中需注明所使用的产品的品牌、规格及型号。"]
["项目包编号：1     项目包名称：激光与通信类实训耗材"]
["序号","品   名","  规   格                             ","数量","单位","备注"]
[1,"激光棒","需带聚焦透镜，直径10~15mm",10,"个"]
[2,"热释电传感器","p228，或者lhi958",20,"个"]
[3,"芯片","BISS0001",20,"块"]
[4,"菲涅尔透镜","与热释电器件配套",50,"个"]
[5,"小车底座","带四轮电机驱动",5,"个"]
[6,"射灯","6V，MR16插口",10,"个"]
[7,"白屏","金属质地，涂白漆，20*20cm，带把手或底座",5,"个"]
[8,"调光相纸/激光调光纸","285*210mm",100,"张"]
[9,"分析纯酒精","99%浓度（500ml）",5,"瓶"]
[10,"搽镜纸","金佰利无尘布擦镜纸",5,"盒"]
[11,"脱脂棉","西光 光学镜头 设备擦拭 长纤维脱脂棉65克±3克/包",3,"包"]
[12,"金属名片","黑（20盒）、金（10盒）、红（10盒）、蓝（10盒）86*54毫米",50,"盒"]
[13,"塑料名片","白色86*54毫米",10,"盒"]
[14,"白卡名片","白色86*54毫米",10,"盒"]
[15,"亚克力板","白色，2m*2m*5mm",2,"张"]
[16,"亚克力板","黑色，2m*2m*5mm",2,"张"]
[17,"亚克力板","红色，2m*2m*6mm",2,"张"]
[18,"二极管","IN4007",200,"个"]
[19,"芯片","电机驱动L293D",10,"块"]
[20,"红外发光对管","红外发光对管",30,"对"]
[21,"芯片","CN3038（dip）",10,"块"]
[22,"继电器","直流，3V，电磁式",30,"个"]
[23,"热敏电阻","NTC，150欧",100,"个"]
[24,"精密滑动变阻器","200欧",50,"个"]
[25,"绝缘垫片","203*122.5cm",21,"块"]
[26,"内六角扳手","Wesser 公制 3mm",1,"个"]
[27,"内六角扳手","Wesser 公制 4mm",1,"个"]
[28,"内六角扳手","Wesser 公制 5mm",1,"个"]
[29,"高级镜头纸","50张/本  10X15CM",10,"本"]
[30,"吹气球","Nisi耐司强力BLOWER 吹气球",1,"个"]
[31,"气嘴","L型螺纹双通  M5XΦ6",10,"个"]
[32,"三极管","3DD15（D880）",100,"个"]
[33,"三极管","3DG12(8050)",100,"个"]
[34,"三极管","3DG6(9014)",100,"个",9014]
[35,"二极管","IN5402",400,"个"]
[36,"稳压管","2DW7A",100,"个","6V/0.5W"]
[37,"电阻","RT14-0.125W-b-2kΩ-±10%",1000,"个","SJ75-73"]
[38,"电阻","RT14-0.125W-b-100Ω-±10%",1000,"个","SJ75-73"]
[39,"电阻","RT14-0.125W-b-120kΩ-±10%",1000,"个","SJ75-73"]
[40,"电阻","RT14-0.125W-b-47kΩ-±10%",1000,"个"]
[41,"电阻","RT14-0.125W-b-560Ω-±10%",1000,"个","SJ75-73"]
[42,"电阻","RT14-0.125W-b-390Ω-±10%",1000,"个","SJ75-73"]
[43,"电阻","RT14-0.125W-b-510Ω-±10%",1000,"个"]
[44,"电阻","RT14-0.125W-b-5.6kΩ-±10%",1000,"个"]
[45,"电阻","RT14-0.125W-b-1.2kΩ-±10%",1000,"个","SJ75-73"]
[46,"可调电阻","WTW470Ω-470Ω-5×6",120,"个"]
[47,"排阻","8×10kΩ",120,"个"]
[48,"电容","CT1-63V-b-0.01uF",1000,"个",103]
[49,"电容","CD11-25-1000uF-SJ803-74",100,"个"]
[50,"电容","CD11-25-100uF-SJ803-74",400,"个"]
[51,"电容","CD11-25-10uF-SJ803-74",400,"个"]
[52,"电路板","三孔或4孔一列，有公共线",200,"块"]
[53,"芯片座","双列直插16脚",400,"个"]
[54,"芯片座","双列直插14脚",100,"个"]
[55,"芯片座","双列直插8脚",100,"个"]
[56,"芯片座","双列直插28脚",100,"个"]
[57,"发光二极管","Φ3",100,"个"]
[58,"芯片","74LS148",50,"个"]
[59,"芯片","74LS279",50,"个"]
[60,"芯片","74LS11",50,"个"]
[61,"芯片","NE555",50,"个"]
[62,"芯片","74LS192",50,"个"]
[63,"贴片收音机套件","ZX2031",100,"个"]
[64,"焊锡丝","质量好、无铅，大卷",10,"卷"]
[65,"交流接触器","CFC2-25/10",20,"个"]
[66,"交流接触器辅助触点","LA1-DN22",20,"个"]
[67,"接线叉","Φ3带绝缘套",5,"包"]
[68,"支架",null,100,"K"]
[69,"银浆","826-1DS",100,"克"]
[70,"绝缘胶","TK303-W",180,"克"]
[71,"环氧树脂","800AB-9","各10","kg"]
[72,"干燥剂","1000pcs",2,"箱"]
[73,"翻晶膜",null,0.5,"卷"]
[74,"模条","φ8",300,"个"]
[75,"模条","φ5",300,"个"]
[76,"脱脂棉",null,3,"包"]
[77,"荧光粉",null,10,"克"]
[78,"LED芯片","普绿（双电极）",100,"K"]
[79,"LED芯片","兰芯（双电极）",100,"K"]
[80,"消泡剂","原材料",1,"小瓶"]
[81,"色素","红色素",0.5,"瓶"]
[82,"扩散剂","DP-090",0.5,"瓶"]
[83,"丙酮",null,10,"kg"]
[84,"金线","1.0mil",2,"卷"]
[85,"单面刀片",null,20,"盒","一盒5片"]
[86,"石膏粉",null,10,"包"]
[87,"白水泥",null,4,"箱"]
[88,"手套","帆布",10,"双"]
[89,"白凡士林",null,1,"公斤"]
[90,"光学玻璃专用胶","每小盒20g，一大盒50小盒",1,"大盒","50小盒"]
[91,"汽油","93＃",5,"升"]
[92,"洗衣粉","3.5kg",3,"袋"]
[93,"排笔",null,200,"支"]
[94,"抛光粉","二氧化铈",5,"公斤"]
[95,"保护漆",null,2,"瓶"]
[96,"抛光柏油","5号",10,"块"]
[97,"抛光柏油","7号",10,"块"]
[98,"橡胶手套","大、中、小号",3,"盒"]
[99,"光学玻璃型料","Φ52.5，d5",200,"块"]
[100,"光学玻璃型料","Φ29.5，d5",200,"块"]
[101,"石膏上盘垫板","φ250 ",2,"块"]
[102,"光学标准板",null,5,"块"]
[103,"SC快速光纤连接器/冷接子","损耗≤0.5dB，回损≥50dB，2.0*3.0蝶形光缆",70,"个"]
[104,"FC快速光纤连接器/冷接子","损耗≤0.5dB，回损≥50dB，2.0*3.0蝶形光缆",70,"个"]
[105,"皮线光缆开剥器","单芯，锌合金，2*3mm",10,"个"]
[106,"皮线光缆光纤定长开剥器导轨条一体","剥涂覆层的跨度为10-30mm，导轨条切割裸纤的跨度为5-40mm",30,"个"]
[107,"单模单芯光纤跳线","SC/SC型，3米，插入损耗≤0.5dB",3,"个"]
[108,"单模单芯光纤跳线","SC/FC型，3米，插入损耗≤0.5dB",3,"个"]
[109,"单模单芯光纤跳线","SC/ST型，3米，插入损耗≤0.5dB",3,"个"]
[110,"单模单芯光纤跳线","FC/FC型，3米，插入损耗≤0.5dB",3,"个"]
[111,"单模单芯光纤跳线","FC/ST型，3米，插入损耗≤0.5dB",3,"个"]
[112,"单模单芯光纤跳线","ST/ST型，3米，插入损耗≤0.5dB",3,"个"]
[113,"光纤热缩套管保护套","60mm，增强不锈钢丝直径1.5mm，热缩管直径3.55mm，热熔管直径2.25mm",200,"个"]
[114,"单模SC散件 2.0","插入损耗≤0.2dB，回波损耗≥55dB，耐用插拔500次",300,"个"]
[115," SC 单摸插芯","陶瓷插带金属尾柄（有防尘帽），与SC散件匹配，同心度 (mm)≤0.002",300,"个"]
[116,"光纤固化胶353ND胶","4g包装（双组份），A:B=10:1，配点胶针筒",4,"个"]
[117,"9μ光纤研磨纸","直径127mm，颗粒9um，适用于光纤跳线陶瓷插芯、连接器端面研磨",5,"个"]
[118,"3μ光纤研磨纸","直径127mm，颗粒3um，适用于光纤跳线陶瓷插芯、连接器端面研磨",5,"个"]
[119,"1μ光纤研磨纸","直径127mm，颗粒1um，适用于光纤跳线陶瓷插芯、连接器端面研磨",5,"个"]
[120,"光纤抛光纸","直径127mm，颗粒0.2um，适用于光纤跳线陶瓷插芯、连接器端面研磨",5,"个"]
[121,"光纤端面研磨机胶垫","适用于中心加压研磨机，硬度80度，直径127mm，5mm",2,"个"]
[122,"三层抽纸","维达超韧系列，软包，3层130抽，家庭装6包",1,"个"]
[123,"光纤接头棘轮 压线钳","TU-301H，硬度HRC45°±3，六角压接工具",10,"个"]
[124,"手动加压喷壶","容量1000ml",2,"个"]
[125,"光纤无尘擦拭纸","40片/袋",50,"个"]
[126,"双头棉花棒","50根/袋",10,"个"]
[127,"多股导线","6平方",2,"卷"]

{"sheet":"电子类","index":1,"n_rows":87,"n_cols":6,"rows_kept":87,"merged":[[0,0,1,5],[3,0,3,5],[4,0,4,4],[79,0,79,5],[80,3,80,4],[81,3,81,4],[82,3,82,4],[83,3,83,4],[84,3,84,4],[85,3,85,4],[86,3,86,4]],"flags":["formulas_cached_only"]}
["电子工程学院实训耗材采购清单、技术规格及要求"]
[]
[]
["投标文件中需注明所使用的产品的品牌、规格及型号。"]
["项目包编号：2     项目包名称：电子类实训耗材"]
["序号","品   名","  规   格                             ","数量","单位","备注"]
[1,"单股导线","1.5平方",45,"卷"]
[2,"绝缘胶带","电工绝缘胶带（卷）",45,"卷"]
[3,"多股导线","2.5平方",5,"卷"]
[4,"九段定时器","套件",450,"套"]
[5,"七管超外差收音机","套件",120,"套"]
[6,"多路波形发生器（手工焊接套件）","人工焊接部分，按套，见附件1",80,"套"]
[7,"丝印辅助件","有铅焊锡膏Sn63，500G/瓶",1,"瓶"]
[8,"丝印辅助件","锡膏稀释剂10ML/瓶",5,"瓶"]
[9,"丝印辅助件","无尘纸：1000张/包",5,"包"]
[10,"万用表套件","MF47A",300,"套"]
[11,"转印纸",null,5,"包"]
[12,"砂纸",null,5,"包"]
[13,"钻头",0.8,10,"盒"]
[14,"钻头",1.2,10,"盒"]
[15,"电脑USB接口与三菱FX系列PLC通讯线","见样",10,"根"]
[16,"导线","φ1.5mm",10,"卷"]
[17,"插针","见样",2,"包"]
[18,"号码管","φ1.5mm",3,"卷"]
[19,"光电开关","CX-441",10,"个"]
[20,"光电开关","MHT15-N2317",5,"个"]
[21,"磁感应式接近开关","D-C73",10,"个"]
[22,"行程开关","见样",5,"个"]
[23,"原点接近开关","见样",2,"个"]
[24,"端子排组件","见样",3,"个"]
[25,"气动阀组","见样",3,"个"]
[26,"电感式接近开关","GH1-305QA",3,"个"]
[27,"金属热电阻",null,3,"个"]
[28,"热敏电阻",null,3,"个"]
[29,"热电偶",null,3,"个"]
[30,"电阻应变式传感器",null,3,"个"]
[31,"压电式传感器",null,3,"个"]
[32,"电感式接近开关",null,3,"个"]
[33,"霍尔传感器",null,3,"个"]
[34,"电容式接近开关",null,3,"个"]
[35,"光电开关",null,3,"个"]
[36,"差动变压器",null,3,"个"]
[37,"湿敏传感器",null,3,"个"]
[38,"气敏传感器",null,3,"个"]
[39,"S7-300 PLC存储卡","6ES7953-8LG20-0AA0",3,"张"]
[40,"光电开关","SICK   VTF18-4P1212",5,"个"]
[41,"行程开关","ME8108 （5A 250VDC  0.4A 115VDC）",5,"个"]
[42,"微动开关","SV-166-1C25（16A 250VAC）",8,"个"]
[43,"直流电机","PM-33246000-200K（24VDC）",5,"台"]
[44,"直流继电器","欧姆龙 MY4NJ（24VDC）",10,"个"]
[45,"指示灯","24V直流指示灯(红、黄、绿)",10,"个"]
[46,"交流电机","220V，25W",2,"台"]
[47,"电涡流传感器","TURCK NI10-Q25-AP6X",2,"个"]
[48,"对讲机",null,2,"个"]
[49,"VGA","视频双公头线",5,"根"]
[50,"USB","转鼠标键盘PLUS接口线",5,"根"]
[51,"钻花","直径2/3/4",10,"个"]
[52,"钻花","直径5/6",10,"个"]
[53,"吸锡器","加热式（40w）",5,"个"]
[54,"双温烙铁","手枪式",1,"个"]
[55,"电热水壶","1.5L",2,"个"]
[56,"万用表表笔","指针式表笔",50,"对"]
[57,"机油壶",null,1,"个"]
[58,"324芯片",null,50,"个"]
[59,"走线槽",null,200,"条"]
[60,"绝缘胶布",null,20,"卷"]
[61,"电阻","1Ω",100,"个"]
[62,"三极管","D880",20,"个"]
[63,"电容",331,50,"个"]
[64,"电池","5号",20,"个"]
[65,"裁纸刀",null,5,"个"]
[66,"恒温烙铁头",null,50,"个"]
[67,"双面胶",null,10,"卷"]
[68,"电位器103",null,20,"个"]
[69,"洗手液",null,3,"瓶"]
[70,"万用表电刷",null,50,"个"]
[71,"单片机电源插口","2.1*5.5mm",50,"个"]
[72,"塑料磨具",null,20,"个"]
[]
["附件1：多路波形发生器(人工焊接部分)"]
["序号","品名","规            格","单板用量",null,"备注"]
[1,"PCB","多路波形发生器,FR4,51*51*1.6mm",1]
[2,"无源晶振","频率:4.19MHz,封装:49SS/SMD,矮体贴片,温漂:±30PPM/℃",1]
[3,"IC","型号:74HC4060,封装:窄体SO-16",1]
[4,"IC","型号:74HC393,封装:窄体SO-14",1]
[5,"贴片钽电容","A型(3216),耐压值:16V,10uF±20%",1]
[6,"三极管","型号:9012,封装:SOT-23",4]

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}