{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["1"],"not_rendered":{"external_links":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"1","index":0,"n_rows":3,"n_cols":4,"rows_kept":3,"merged":[[2,0,2,3]],"flags":["formulas_cached_only"]}
["产品/工程名称","技术参数","单位","数量"]
["P3.91LED租赁屏","像数点间距：≤3.91mm\n像素密度：65536Dots/㎡\n结构特点：灯驱合一\n箱体框规格：500mm*1000mm\n驱动方式：1/16 动态恒流驱动\n亮度：≥800cd/㎡\n亮度均匀性：＞0.95\n屏幕水平视角：140±10°\n屏幕垂直视角：130±10°\n最佳视距：≥3.91\n最大功耗：≤509.76W/㎡\n配电功率（每平方最大功率÷78%÷85%）：768.87W\n使用环境：室内\n灰度等级：红、绿、蓝各 12-16bits\n显示颜色：43980 亿种\n换帧频率：≥60 帧/秒\n刷新频率：≥3840Hz\n控制方式：计算机控制，逐点一一对应，视频同步，实时显示\n亮度调节：256 级手动/自动\n输入信号：DVI/VGA，视频(多种制式)；RGBHV、复合视频信号、S-VIDEO YpbPr(HDTV)\n使用寿命：≥10 万小时\n平均无故障时间：≥1 万小时\n衰减率(工作 3 年)：≤15％\n连续失控点：0\n离散失控点：＜0.0001，出厂时为 0\n盲点率：＜0.0001，出厂时为 0\n工作温度范围：-20 至 50℃\n工作湿度范围：10％至 65％RH\n防护性能：超温/过载/掉电/图像补偿/各种校正技术/过流/过压/防雷(可选项)\n屏幕水平平整度：＜1mm/㎡\n屏幕垂直平整度：＜1mm/㎡","㎡",24]
["注：请在投标文件中明确指出所投产品的品牌、规格、型号"]