{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":20,"n_cols":6,"rows_kept":20,"merged":[[0,0,0,5],[1,1,1,2],[2,0,2,5],[3,1,3,2],[4,1,4,2],[5,1,5,2],[6,1,6,2],[7,1,7,2],[8,1,8,2],[9,1,9,2],[10,0,10,5],[11,1,11,2],[12,1,12,2],[13,1,13,2],[14,1,14,2],[15,1,15,2],[16,1,16,2],[17,1,17,2],[18,1,18,2],[19,0,19,3]],"flags":["formulas_cached_only"]}
["体育馆屋面防水工程量清单"]
["序号",null,null,"规格型号","单位","数量"]
["一、主要材料"]
[1,"防水型丙烯酸酯涂料（国内一线品牌）",null,992,"㎡",400]
[2,"防水型丙烯酸酯涂料（国内一线品牌）",null,991,"㎡",400]
[3,"聚氨酯防水涂料(国内一线品牌)",null,null,"㎡",1200]
[4,"无纺布（国内一线品牌）",null,null,"m",400]
[5,"槽钢10#",null,"10#","m",150]
[6,"角钢10#",null,"10#","m",60]
[7]
["二、施工费用"]
[1,"焊接上下楼梯及加装护栏，涂刷防锈油漆两遍",null,null,"项","30工日"]
[2,"清理屋面所有天沟内积水及渣滓",null,null,"㎡",400]
[3,"铲除天沟内及四周所有老化基层",null,null,"㎡",400]
[4,"992防水型丙烯酸酯涂料封面",null,null,"㎡",400]
[5,"聚氨酯防水涂料进行三次涂刷",null,null,"㎡",1200]
[6,"用无纺布进行边角加强防水处理",null,null,"㎡",400]
[7,"用991丙烯酸酯弹性乳胶进行防水处理",null,null,"㎡",400]
[8,"租赁脚手架"]
["注：请在投标文件中明确指出所使用材料的品牌、规格及型号"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}