{"text_format":"3","workbook":"xls","n_sheets":2,"sheets":["分部分项工程和单价措施项目清单综合单价分析表","Sheet1"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"分部分项工程和单价措施项目清单综合单价分析表","index":0,"n_rows":21,"n_cols":5,"rows_kept":21,"merged":[[0,0,0,4],[1,0,1,4],[2,0,2,4],[3,0,3,4],[4,0,4,4],[6,0,11,0],[6,1,11,1],[6,2,11,2],[6,3,11,3],[6,4,11,4],[12,0,14,0],[12,1,14,1],[12,2,14,2],[12,3,14,3],[12,4,14,4],[15,0,16,0],[15,1,16,1],[15,2,16,2],[15,3,16,3],[15,4,16,4],[17,0,18,0],[17,1,18,1],[17,2,18,2],[17,3,18,3],[17,4,18,4]],"flags":["formulas_cached_only"]}
["1、2#教学楼天井增加玻璃雨棚建设项目清单，技术规格、参数及要求","",null,"",""]
["注：投标文件中需注明货物的品牌、型号、规格与详细技术参数等。","",null,"",""]
["一、顶盖做法"]
["1.钢龙骨为80*60*4镀锌方钢管，刷防锈漆二遍，刷氟碳二遍\n2.玻璃为夹胶钢化玻璃8+1.52PVB+8\n3.预埋钢板为200*200*10 化学螺栓固定在结构上                                                                               4.顶盖采用平顶方式，坡度2-3%"]
["二、分项清单"]
["序号","工程项目名称","项目描述","单位","数量 "]
[1,"8+1.14PVB+8双钢化夹胶玻璃屋面","1.骨架材料种类、规格:中距:1200MM*1800MM间距.Q235B碳素钢80*60*4镀锌方管钢龙骨，；立柱80*60*4镀锌方管平均高0.6米，间距为1.2米；立柱焊接固定在预埋钢板上；金属结构表面刷氟碳喷涂处理；漆膜达到国标要求；\n2.玻璃品种、规格、颜色:8+1.14PVB+8双钢化夹胶玻璃\n3.粘结塞口材料种类:结构胶\n4.固定方式:结构胶粘贴                                             5.屋顶成品保护","㎡",470]
[]
[]
[]
[]
[]
[2,"预埋铁件","1、钢材种类Q223\n2、规格；龙骨底座10MM厚铁板\n3、铁件尺寸；200MM*200MM；M16化学螺栓固定\n4、防锈底漆二道，表面刷氟碳漆","t",0.5]
[]
[]
[3,"墙面喷刷涂料","1、表面铲除饰面涂料及水泥修补\n2、重新刷外墙涂料","㎡",285.6]
[]
[4,"脚手架","自行考虑；决算不再调整；包括钢结构安装玻璃屋顶安装等所有搭设及拆除用的脚手架；对学生保护用通道脚手架","项",1]
[]
[5,"建筑垃圾外运","所有建筑人工搬运及装车外运","项",1]
[6,"材料搬运上楼","建筑项目所有材料搬运至屋顶","项",1]

{"sheet":"Sheet1","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}