{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":27,"n_cols":6,"rows_kept":27,"merged":[[0,0,0,5],[1,0,1,5],[2,0,2,5],[4,5,5,5],[6,0,6,5],[29,3,29,5]],"flags":["formulas_cached_only"]}
["汉口校区一楼大厅填平及七楼厕所改造建设项目\n工程量清单，技术规格、参数及要求\n"]
["投标文件中需注明所使用的产品的品牌、规格及型号。"]
["一、一楼大厅填平"]
["序号","项目名称","规格","计量单位","工程量","备注"]
[1,"地面混凝土填平",null,"㎡",73,"面积73平米，高26厘米。           工艺上注意与原其他地面衔接协调"]
[2,"填平后铺砖","玻化砖600×600","㎡",73]
["二、七楼厕所改造建设"]
[3,"卫生间（男女）含淋浴房一间","长7m，宽4.5m","㎡",31.5,"蹲坑墙面1m高，淋浴房墙面2m高"]
[4,"淋浴房及配套设施",null,"套",2]
[5,"地砖",null,"㎡",32]
[6,"墙砖",null,"㎡",107]
[7,"蹲便器及配件安装",null,"套",6,"二线以上品牌"]
[8,"隔断","埃特板","档",6]
[9,"洗手台及配套设施",null,"套",3,"二线以上品牌"]
[10,"地面墙面防水层",null,"㎡",72]
[11,"吊顶","铝扣板","㎡",32,"材料厚度不低于0.6mm"]
[12,"更换门",null,"套",2]
[13,"更换窗",null,"套",2]
[14,"不锈钢地漏",null,"个",6]
[15,"开关插座",null,"个",8,"一线品牌"]
[16,"砖砌蹲台","砖砌蹲台","㎡",2.5]
[17,"蹲台回填土","蹲台回填土","m³",3.5]
[18,"给水管","PPR","m",90]
[19,"排水管","pvc","m",45]
[20,"电线",null,"m",260]
[21,"拆除渣土转运下楼","七层","㎡",33]
[22,"人工搬运材料上楼","七层","㎡",45]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}