{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":60,"n_cols":8,"rows_kept":60,"merged":[[0,0,0,7],[1,3,1,4],[2,3,2,4],[3,3,3,4],[4,3,4,4],[5,3,5,4],[6,3,6,4],[7,3,7,4],[8,3,8,4],[9,3,9,4],[10,3,10,4],[11,3,11,4],[13,0,13,7],[14,3,14,4],[15,3,15,4],[16,3,16,4],[17,3,17,4],[18,3,18,4],[19,3,19,4],[20,3,20,4],[21,3,21,4],[22,3,22,4],[23,3,23,4],[26,0,26,7],[27,3,27,4],[28,3,28,4],[29,3,29,4],[30,3,30,4],[31,3,31,4],[32,3,32,4],[33,3,33,4],[34,3,34,4],[35,3,35,4],[36,3,36,4],[37,3,37,4],[38,3,38,4],[39,3,39,4],[40,3,40,4],[41,3,41,4],[42,3,42,4],[43,3,43,4],[44,3,44,4],[45,3,45,4],[46,3,46,4],[47,3,47,4],[48,3,48,4],[49,3,49,4],[50,3,50,4],[51,3,51,4],[52,3,52,4],[53,3,53,4],[54,3,54,4],[55,3,55,4],[56,3,56,4],[57,3,57,4],[58,3,58,4],[59,3,59,4]],"flags":["formulas_cached_only"]}
["商学院实训室防盗门安装及电路改造工程量清单"]
["序号",null,"项目名称","项目特征描述",null,"计量单位","工程量","备注"]
[1,null,"防盗门","1㎜厚，尺寸1*2.1*31个；1.3*2.1*23个  ",null,"㎡",127.89,"投标文件中需注明防盗门品牌"]
[2,null,"五孔插座（设备用","明装",null,"个",402]
[3,null,"3P柜机空调空开","明装",null,"个",74]
[4,null,"室内空开箱 ","DZ47-3P-60A",null,"台",24]
[5,null,"室内空开箱","DZ47-3P-32A",null,"台",6]
[6,null,"4㎜2单芯铜线","武汉二厂电线设备插座用",null,"m",11280]
[7,null,"6㎜2单芯铜线","武汉二厂电线空调用",null,"m",3400]
[8,null,"开槽及水泥砂浆铺设恢复",null,null,"m",4893]
[9,null,"日光灯清洗",null,null,"套",327]
[10,null,"吊风扇清洗 ",null,null,"台",160]
[]
["商学院光谷银行实训室装修改造工程量清单"]
["序号",null,"项目名称","项目特征描述",null,"计量单位","工程量","备注"]
[1,null,"柜台玻璃隔断","12mm钢化玻璃隔断",null,"㎡",15]
[2,null,"饰面","钢结构骨架木芯板基层铝塑板饰面（分隔墙）",null,"㎡",33]
[3,null,"饰面","吊楣钢结构骨架木芯板肋板木芯板基层铝塑板饰面",null,"㎡",14.46]
[4,null,"饰面","木芯板肋板龙骨木芯板基层灰色防火板饰面",null,"㎡",4.08]
[5,null,"传钞斗","不锈钢传钞斗（350*200*150）",null,"个",4]
[6,null,"台面","深灰色色丽石台面",null,"㎡",7.38]
[7,null,"PVC20线管","PVC20线管",null,"m",50]
[8,null,"电气配线BV—4MM2","电气配线BV—4MM2",null,"m",120]
[9,null,"插座面板",null,null,"个",5]
[]
[]
["环境与生化工程学院实训室改造工程量清单"]
["序号",null,"项目名称","项目特征描述",null,"计量单位","工程量","备注"]
[1,null,"新增白板",null,null,"㎡",4.8]
[2,null,"金属装饰线","不锈钢阳角线",null,"m",80]
[3,null,"钢制防盗门","钢制防盗门（1.3*2.15*2）",null,"㎡",5.59,"投标文件中需注明防盗门品牌"]
[4,null,"隔墙块料墙面","250*330",null,"㎡",18.36]
[5,null,"拆除实木门铁门","1.35*2.15",null,"樘",4]
[6,null,"金属（塑钢）门",null,null,"㎡",2.44]
[7,null,"块料墙面","250*330",null,"㎡",98.5]
[8,null,"六孔插座",null,null,"套",21]
[9,null,"空调插座",null,null,"套",1]
[10,null,"双开",null,null,"个",3]
[11,null,"电气配管","PVC20线管",null,"m",300]
[12,null,"空开盒",null,null,"个",5]
[13,null,"总空开箱","500*600",null,"个",1]
[14,null,"吊顶格栅灯","600*600",null,"套",15]
[15,null,"电气配线","6mm2单芯护套线",null,"m",350]
[16,null,"电气配线","4mm2单芯护套线",null,"m",450]
[17,null,"电气配线","2.5mm2单芯护套线",null,"m",400]
[18,null,"100A3P空开","100A3P空开",null,"个",1]
[19,null,"60A2P空开","60A2P空开（带漏宝）",null,"个",1]
[20,null,"32A2P空开","32A2P空开（带漏宝）",null,"个",11]
[21,null,"16A1P空开","16A1P空开",null,"个",2]
[22,null,"电力电缆","3*35+2*16",null,"m",35]
[23,null,"墙面开槽及恢复",null,null,"m",608]
[24,null,"开墙洞","0.6*0.5m",null,"个",1]
[25,null,"塑料管","PPR25",null,"m",35]
[26,null,"塑料管","PVC75",null,"m",30]
[27,null,"塑料阀门","Φ25总阀",null,"个",1]
[28,null,"塑料阀门","三角水阀",null,"个",6]
[29,null,"塑料阀","Φ25分水阀",null,"个",1]
[30,null,"水龙头",null,null,"个",1]
[31,null,"成品拖把池","成品拖把池（大）",null,"个",1]
[32,null,"塑钢纱窗",null,null,"㎡",8.5]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}